# Visual outputs of the Voith gear range selector E330 Any occurring faults are indicated to the driver by blinking gear range selector lights. The different blinking codes inform about type and priority of the fault. This function is available as of gear range selector switch version G01.03. The software version is displayed in the Identification data in the ALADIN ECU Report.
| E330 blinking codes
> Fault type or priority | Blinking duration | Blinking keys | Blinking frequency | Ratio of lighting ON / OFF | Start animation
> CAN fault The gear range selector has no communication on the CAN bus. (no connection between gear range selector and transmission control unit) | Until ignition is off | All | 1 Hz (once per second) | 1 / 1 |
> Priority 1 event (saved) The event memory of the transmission control unit signals one priority 1 fault saved after the ignition has been switched on. | 10 seconds | All | 2 Hz (twice per second) | 1 / 1 |
> Priority 2 event (saved) The event memory of the transmission control unit signals one priority 2 fault saved after the ignition has been switched on. | 10 seconds | All | 2 Hz (twice per second) | 1 / 1 |
> Priority 1 event (current) The transmission control unit signals one currently active priority 1 fault. | Until ignition is off | All | 2 Hz (twice per second) | 1 / 1 |
> Priority 2 event (current) The transmission control unit signals one currently active priority 2 fault. | 10 seconds | All | 2 Hz (twice per second) | 1 / 1 |
> Priority 6 event (current) The transmission control unit signals one currently active priority 6 fault. | Until ignition is off or fault is eliminated | "N" button | 1 Hz (once per second) | 1 / 3 |
> The transmission control unit refuses to accept gear | As long as button is pushed in or until gear is accepted | Pushed-in button | 1 Hz (once per second) | 1 / 1 |
Up > Higher-level section © by Voith Turbo GmbH & Co. KG send remarks to joachim.ehleiter@voith.com (electronic department) or r.theilacker@voith.com (electronic department)