Start page To favorites Print page |

### Service - Pushbutton selector

The pushbutton selector depicted indicates whether and which button is currently recognized by the transmission controller as pressed. The pressed button is highlighted in color. If no button switch is detected, all buttons depicted appear on a gray background. If a pushbutton selector is not detected by the transmission controller, carry out an upload for targeted troubleshooting.

Engaging a gear range key (1, 2, 3, D and R) only means that driving is intended. This intention to drive is displayed here in the window. The transmission controller also checks whether this intention to drive can be accepted. The real pushbutton selector has several flashing codes that indicate the refusal of engaging gears, for example. The flashing codes are not displayed in the window.

## Valid platforms:

- DIWA.3 via E200
- DIWA.3 via E310
- DIWA.5
- DIWA.6 via KWP
- DIWAhybrid E300.1

The pushbutton selector is accessed via the Service group in the main window. Then select the pushbutton selector button in the Service menu.

The pushbutton selector is offered depending on the connected ECU. No functions are available without communication.

The display changes automatically after you have started the communication.