Start page To favorites Print page |

### Trace window

The Trace window contains messages on the communication with a connected controller. This includes debug messages and configuration settings for the communication and the pure communication data between the interface and the controller.
In the default settings only debug messages are displayed. The recording of the communication trace between ALADIN and a controller is very performance-intensive and must therefore be specifically activated in the ALADIN settings.

The Trace window is used for specific troubleshooting in the controllers' communication and for the controllers' development.

## Valid platforms:

- DIWA.3 via E200
- DIWA.3 via E310
- DIWA.5
- DIWA.6 via KWP
- DIWA.6 via UDS
- VIAB
- DIWAhybrid E300.1
- DIWAhybrid M300

In the communication trace, as in any editor - you can add texts, delete texts or copy and paste using the "CTRL+c" and "CTRL+v" keyboard combinations.
You can use the "Diskette symbol" button to save all the text from the Response area in TXT format.
You can use the "Trash can symbol" button to delete the entire content in the Response area.
The "Auto-Delete" function deletes the trace after 100 entries.
The "Additional information" function can be used to switch the tracing of debug information on and off. If "Additional information" is switched off and the communication trace in the ALADIN setting is also switched off, there are no entries in the trace.