Engine control unit - VDO E-gas
|  | Terminal connection diagram
|  | Test steps
|  | See also:
Terminal connection diagram Test steps Open S2 plug connection (cable 2). Measure resistance between contact 41 and corresponding contact at engine control unit (PWM output). RTarget = 0 Ω. Check resistance of contact 41 (cable 2) to vehicle ground. RTarget = ∞ Ω. See also:
|  | Engine control unit test - CAN SAE J1939 / IES
© by Voith Turbo GmbH & Co. KG send remarks to markus.zwickel@voith.com (documentation department)