Unknown engine load source Unknown engine load source
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
Description Unknown engine load source. Effects on the driving operation The engine torque reduction does not enable shifts, since neither the current nor the maximum engine torque are available. Tehrefore noe shifts are executed. Possible causes The dataset value ENG_ECU_TYPE_ is faulty. Possible values are: 1 - Engine load source CAN 2 - Engine load source CAN Place of action No description available. Instruction Load correct dataset. Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)