CAN-pushbutton switch E330 Inadmissible conditions at the output
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
Description Inadmissible states have been detected while monitoring the flexible output. Effects on the driving operation The flexible output at the gear range selector is non-functional. Possible causes Hardware fault of the gear range selector or the transmission control unit. Place of action No description available. Instruction Clear fault memory and retest the gear range selector. Should the fault reoccur, please contact the VOITH customer service. Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)