Software module Event memory Data set value EVENTMEM_DELETE_ELEMENT_AFTER_ faulty
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
Description The dataset value EVENTMEM_DELETE_ELEMENT_AFTER_ is incorrectly set to 0. The event memory would be cleared as a consequence after each system start. Therefore, the software has blocked the automatic, time-dependent clearing Effects on the driving operation The software has blocked the automatic, time-dependent deletion of the data. Possible causes Faulty dataset or dataset value EVENTMEM_DELETE_ELEMENT_AFTER_ was modified illegally. Place of action No description available. Instruction Load appropriate dataset. Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)