Transmission mechanism slip monitoring Disk slip in mechanical gear.
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Location
|  | Instruction
|  | Setting conditions for the event
|  | Test conditions for the event
|  | Final function check
Description Disk slip in mechanical gear. Effects on the driving operation No driving. Tractive power drop. "Racing" engine speed. Possible causes Low oil level, low operating pressure, defective piston ring, defectiv disks. Location Engine speed sensor (negative terminal of sensor or sensor circuit) Instruction Check oil level, operating pressure, piston rings and disks. Setting conditions for the event No description available. Test conditions for the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)