Engine speed sensor Undiagnosable fault
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Test conditions of the event
|  | See also:
Description Undiagnosable fault. Effects on the driving operation Hard shifts Driving in reverse gear is not possible or restricted. If the output sensor is also defective, only limp-home mode available No torque limitation relative to the engine speed Engine torque reduction is limited. The characteristic curve of the auxiliaries is not considered. The engine speed and values derived from it are incorrectly set in the CAN communication. Possible causes No description available. Place of action Engine speed sensor Instruction No description available. Setting conditions of the event No description available. Test conditions of the event No description available. See also:
|  | Aftersales service index
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)