Transmission mechanism slip monitoring Unknown slip protector mode
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Location
|  | Instruction
|  | Setting conditions for the event
|  | Test conditions for the event
|  | Final function check
Description Unknown slip protector mode Effects on the driving operation Transmission damage, because no protective measures have been taken. Possible causes The dataset constant SLIP_PROTECTOR_MODE_ contains a faulty value. The software version does not support the protective measures specified in the dataset. Location Engine speed sensor (negative terminal of sensor or sensor circuit) Instruction Load correct combination of dataset and software. Setting conditions for the event No description available. Test conditions for the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)