Software module Event memory Fault in dataset
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Troubleshooting
|  | Instruction
|  | Setting conditions of the event
|  | Test conditions of the event
|  | Final function check
|  | See also:
Description The data dataset value EVENTMEM_TIME_UNTIL_DELETE_ is incorrectly set to 0. The event memory would be cleared as a consequence after each system start. Therefore, the software has blocked the automatic, time-dependent clearing Effects on the driving operation The software has blocked the automatic, time-dependent deletion of the data. Possible causes Faulty dataset or dataset value EVENTMEM_TIME_UNTIL_DELETE_ was modified illegally. Place of action No description available. Troubleshooting
|  | NOTE The following service work may only be performed by persons who are authorised by the vehicle manufacturer: Loading software and/or datasets into the transmission control unit. Service work at vehicle components which are not included in the VOITH delivery.
Instruction Load appropriate dataset. Setting conditions of the event No description available. Test conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test the function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read out the fault memory. Check the transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions. See also:
|  | Aftersales service index
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)