Engine speed sensor Undiagnosable fault
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
Description Unknown fault. Effects on the driving operation Hard shifts. No switching into reverse gear. Main pressure to maximum. Reduction of the engine torque to protect the transmission. If the engine transmission output speed sensor is simultaneously defective, only limp-home mode available. The engine speed and/or the values derived on its basis are incorrectly set in the CAN communication. Possible causes No description available. Place of action Engine speed sensor Instruction No description available. Setting conditions of the event No description available. Testing conditions of the event No description available.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)