Software module Identification Data Invalid identifier: software production date
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Testing conditions of the event
|  | Final function check
Description Invalid identifier: software production date Effects on the driving operation No description available. Possible causes At least one of the production date(s) read out of the (transmission) function software/safety computer software is invalid. The value was either overwritten or incorrectly entered. The valid format is YYYY-MM-DD, saved as 4BCD value The (transmission) function software has entered the default value 0000-00-00. Place of action No description available. Instruction Please contact the VOITH customer service. You need a different software version. Setting conditions of the event No description available. Testing conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read the fault memory Check transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions correctly.
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)