Start page To favorites Print page |

### Service - Load transducer

The load transducer test provides information on which accelerator pedal position is active.

## Valid platforms:

- DIWA.3 via E200
- DIWA.3 via E310
- DIWA.5
- DIWA.6 via KWP
- DIWAhybrid E300.1

## How to open the load transducer test

The load transducer test is accessed via the Service group in the main window. Then select the Load transducer button in the Service menu.

The load transducer test is offered depending on the connected ECU. The load transducer test is not available without communication.

The display changes automatically after you have started the communication.