CAN gear range selector E330 The oscillator watchdog has triggered a reset.
|  | Description
|  | Effects on the driving operation
|  | Possible causes
|  | Place of action
|  | Instruction
|  | Setting conditions of the event
|  | Test conditions of the event
|  | Final function check
|  | See also:
Description An internal hardware fault has occurred in the CAN gear range selector: The oscillator watchdog has triggered a reset. Effects on the driving operation Driving is no longer possible. The transmission shifts to neutral. All buttons on the gear range selector are flashing. The limp-home switch allows activating the limp-home mode. Possible causes Gear range selector defective. Place of action No description available. Instruction Replace gear range selector. Setting conditions of the event No description available. Test conditions of the event No description available. Final function check If the defective component cannot be clearly identified, you should try to reproduce the fault: Reinstall the component in the vehicle. Test the function. After the fault has been eliminated, the following steps have to be carried out: Conduct a test drive with function check. Read out the fault memory. Check the transmission for leaks. Perform a final visual inspection. These steps are necessary to ensure the entire vehicle functions. See also:
|  | Aftersales service index
© by Voith Turbo GmbH & Co. KG, S. Brunnengräber send remarks to stefan.brunnengraeber@voith.com (documentation department)