# The Boot / Flash Loader The Flash Loader is a software in the transmission control unit that is responsible exclusively for loading function software and datasets. It is therefore necessary for putting a transmission control unit into operation. The loader designation starts with an "F" (for "flash"), followed by the version number: There are also loader updates that are marked with '-u' in addition to the version. Valid loaders are:
Transmission control unit | Loader |
E300 | F04.04.07-u |
E300.1 | F05.05.03-u |
E300.1 | F05.08.00-u |
| Further topics:
More information on: Dataset More information on: Function software More information on: The Intel hex format More information on: Download More information on: FAQ More information on: ALADIN terms Up > [Linkleisten stehen auf dieser Website nicht zur Verfügung] © by Voith Turbo GmbH & Co. KG send remarks to joachim.ehleiter@voith.com (electronic department) or r.theilacker@voith.com (electronic department)