# Display service data in the report
| The service data area displays all the service data that has been entered in the control unit. Service data is used to optimize services, allocate an ECU file to a service case and to manage the ECU data in the central Voith database. The service data has been entered by the Voith customer service during the pre-delivery inspection (PDI) of the bus. If you have to make any modifications in the service data, click Service in the main window.
| Service data report contents:
> |  | Service data can have the following data fields:
> |  | Vehicle:
> Data field | Notes | Example |
> Vehicle manufacturer |  | MAN |
> Vehicle type designation | Designation assigned by the vehicle manufacturer | A22 |
> Vehicle model |  | Midibus |
> Chassis number | Number for the unambiguous identification of a vehicle. Identical to the vehicle identification number. | WMAA22ZZ06C00599 |
> Vehicle Identification Number (VIN) | The vehicle identification number replaces the former chassis number. For further information, please see: VIN | WMAA22ZZ06C00599 |
> Bus number | Number assigned by the vehicle manufacturer. Similar to a serial number. | A221820 |
> Commissioning date | Date in European format (DD.MM.YYYY). | 15.03.2006 |
> Curb weight | In kilograms | 12000 |
> Maximum speed | In km/h | 100 |
> Vehicle application | The vehicle application differentiates between cross-country traffic and city traffic. City traffic is divided into three SORT levels. For further information, please see: SORT | City traffic (SORT2) |
> Topography | Topography describes the terrain in which the vehicle is mainly used. The terrain is divided into: plane slightly hilly hilly mountainous . | Plane |
> Tyre type | Tyre type of the driving wheels | 275 / 70 R 22.5 |
> Axle ratio | Transmission ratio of the drive axle | I:5.74 |
> |  | For modifications in the vehicle data, please see: Service data – vehicle.
> |  | Engine:
> Data field | Notes | Example |
> Engine manufacturer |  | MAN |
> Engine type designation | Designation assigned by the vehicle manufacturer | D 2866 LUH 13 |
> Max. torque | In Nm (Newton meters) | 950 |
> Power | in kW (kilowatts) | 180 |
> Nominal speed | In rpm (rotations/minute) | 2400 |
> Cubic capacity | In cm³ (cubic centimeters) | 6500 |
> Number of cylinders |  | 6 |
> Exhaust emission standard |  | Euro 3 |
> |  | For modifications in the engine data, please see: Service data – engine.
> |  | Transmission:
> Data field | Notes | Example |
> Transmission serial number |  | 500350 |
> Transmission type | The DIWA.5 transmission type | D864.5 |
> Transmission model | For further information, please see: DIWA.5 designs and types. | D4HT0R2-6.5 |
> Transmission type | For further information, please see: DIWA.5 designs and types. | 66.7921.1 |
> Transmission version | For further information, please see: DIWA.5 designs and types. | 152.00064610 |
> Oil manufacturer (60,000 km) | For the DIWA.5 transmission, there are approved lubricants for normal oil change intervals (every 60,000 km) and for extended oil change intervals (every 120,000 km). For information on approved lubricants for normal oil change intervals, please refer to: Lubricant chart H55.633534. For information on approved lubricants for extended oil change intervals, please refer to: Lubricant chart H55.633634. | Shell |
> Oil type (60,000 km) | See oil manufacturer (60,000 km). | Donax TG |
> Oil manufacturer (120,000 km) | See oil manufacturer (60,000 km). | Shell |
> Oil type (120,000 km) | See oil manufacturer (60,000 km). | Donax TX |
> |  | For modifications in the transmission data, please see: Service data – transmission.
> |  | Customer:
> Data field | Notes | Example |
> Customer | Name / company name of the customer | Public transportation services Demo City |
> Country | Country where the customer is located | Germany |
> Town/place | Town where the customer is located | Demo City |
> Contact | Name of the contact person at the customer's | John Doe |
> Phone | Phone number of the contact person (always with country and local code) | 0049 8321 6874 |
> E-mail | e-mail address of the contact person | John.Doe@customer.com |
> Bus number | Bus identifier assigned by the customer | No. 25 |
> Depot | Vehicle location at the customer's | Depot, Demo street |
> Registration number | Text of the licence plate | M XYZ 123 |
> Warranty code | Identification of the warranty type granted for this vehicle by Voith |  |
> |  | For modifications in the customer data, please see: Service data – customer.
> |  | Service:
> Data field | Notes | Example |
> Service provider | Name of the Voith service office responsible for this transmission For information on Voith service offices, please see the Customer service index. | Voith Turbo S.A. / N.V. |
> Processor | Name of the responsible Voith service employee | John Doe |
> Phone | Phone number of the Voith service employee / Voith service office (always with country and local code) | 0049 7321 1234 |
> E-mail | e-mail address of the Voith service employee / Voith service office | John.Doe@Voith.com |
> Installation location of control unit | Description where the control unit is located in the vehicle | Behind the driver's workplace |
> Installation location of diagnosis terminal | Description where the central diagnosis port is located in the vehicle (if applicable) | To the right of the front door |
> |  | For modifications in the service data, please see: Service data – service.
> |  | Additional service information:
> Data field | Notes | Example |
> Comment / problem description | Information that might be helpful in service case. Who has done what, why and where. | Name of the VOITH employee Date of the service visit Reason of the service visit Problems that occurred Actions carried out |
> Data fields for service data not entered are not displayed. If no service data is entered in the transmission control unit, the message: "No service data available!". In this case, please have the service data entered by your Voith customer service responsible.
| How to adjust the report contents:
In the ALADIN Setup, you can configure what is displayed and how it is displayed in the ECU report. Click Setup > Report in the main window. For further information, please see: Report setup.
| How to modify service data:
If you want to modify the service data, click Service in the main window. For further information, please see: Service data.
| How to delete service data:
If you want to delete individual service data in the transmission control unit, edit the corresponding input fields in the "Service data" window and then save the changes using the Write to ECU button. For further information, please see: Service data. If you want to delete the complete information in the transmission control unit, carry out a reset. For this purpose, select Service > Reset functions > Delete service data in the main window. For further information, please see: Reset functions.
| How to save service data on your PC:
You can use a so-called template to save the service data entered as a .hex file on your PC. For further information, please see: Template.
| Further topics:
More information on: Upload More information on: User level More information on: main window. More information on: DIWA.5 design and rating plate More information on: SORT More information on: VIN More information on: Voith customer service index More information on: Setup More information on: FAQ Up > [Hyperlinkleisten stehen auf dieser Website nicht zur Verfügung] © by Voith Turbo GmbH & Co. KG send remarks to joachim.ehleiter@voith.com (electronic department) or r.theilacker@voith.com (electronic department)