# Setup - EOL tab In the EOL tab, you can set the columns to be displayed in the Voith EOL Manager. For information on the EOL Manager, please see: Voith EOL Manager.
| The ALADIN Setup default settings correspond to the diagnostic tasks of the 'Customer' and 'Service' user levels!
| How to open the Setup window:
> | Click Setup in the ALADIN main window.
| How to save in the Setup window:
> | Click the Exit button in the Setup window. The dialog "Save ALADIN Setup" appears. Click Yes if you want to accept the settings in the Setup. Click No if you want to discard the changes.
| You can activate the following EOL columns:
> | Report section | Description |
> | Byte | Developer information |
> | Byte start position | Developer information |
> | Byte length | Developer information |
> | Bit | Developer information |
> | Bit start position | Developer information |
> | Bit length | Developer information |
> | Value has been changed | Developer information |
> | Parameter is ReadOnly | Developer information |
> | Value state | Displays the status of the EOL value. (OK, available, fault identification) |
> | Value in HEX | Displays the EOL values in hexadecimal notation. |
| Further topics:
More information on: EOL More information on: EOL in the report More information on: FAQ Up > Higher-level section © by Voith Turbo GmbH & Co. KG send remarks to joachim.ehleiter@voith.com (electronic department) or r.theilacker@voith.com (electronic department)