# SORT display
| SORT is a project between bus carriers and manufacturers for developing standardized fuel consumption tests for buses. Apart from factors such as the loading status of a vehicle, the vehicle application is decisive for fuel consumption. SORT defines three different application scenarios (SORT cycles) for buses: SORT 1 to SORT3. For further information on SORT, please see: SORT. The ECU displays what SORT cycle a vehicle can be assigned to.
| SORT report contents:
> | The display of the SORT cycles:
> | The possible allocation of a vehicle to a SORT cycle is displayed in three charts: The stops per kilometer based on the average speed The percentage of stop times based on the average speed The stops per kilometer based on the percentage of stop times
> Symbol | SORT cycle | Description
> | Reference point SORT 1 | According to definition for heavy city traffic
> | Reference point SORT 2 | According to definition for light city traffic
> | Reference point SORT 3 | According to definition for suburban traffic
> | This vehicle |
> For further detailed information on SORT cycles, please see: SORT.
> | Display example:
> | The charts indicate that this vehicle is to be classified between the two SORT2 and SORT3 cycles.
| How to adjust the report contents:
In the ALADIN Setup, you can configure what is displayed and how it is displayed in the ECU report. Click Setup > Report in the main window. For further information, please see: Report setup.
| Further topics:
More information on: Upload More information on: Setup More information on: SORT Up > Higher-level section © by Voith Turbo GmbH & Co. KG send remarks to joachim.ehleiter@voith.com (electronic department) or r.theilacker@voith.com (electronic department)