# The dataset The software in the transmission control unit comprises of three parts: a function software, a dataset and a Boot Loader. The purpose of the dataset is configuring the functions of the transmission software. The dataset is used, for example, to configure shift programs, define calculation values, configure flexible inputs / outputs or define CAN receive messages. In short: The function software defines how something is calculated, the dataset includes the values for calculation. A complete dataset comprises approx. 1,000 different configuration variables. The complete name of a dataset includes the identifier of the corresponding function software that consists of the version and the appropriate hardware, a dataset identifier and the file extension ".hex". A dataset for the E300.1-D5.2.0.0 software with the dataset identifier "08154711" would have the following name: E300.1-D5.2.0.0-08154711.hex. With this type of designation, you can see from the name what combination of hardware, software and dataset goes together. In the event that a dataset must be adapted, e.g., because of missing or wrong CAN receive messages, please contact the Voith customer service.
| With transmission unit software version D5.8.0.0 and higher, dataset values can be defined by EOL parameters.
| Further topics:
More information on: EOL More information on: Download More information on: Function software More information on: The Intel hex format More information on: Scourcer More information on: ECU report dataset analysis More information on: Boot / Flash Loader More information on: FAQ More information on: ALADIN terms More information on: Voith customer service Up > Higher-level section © by Voith Turbo GmbH & Co. KG send remarks to joachim.ehleiter@voith.com (electronic department) or r.theilacker@voith.com (electronic department)