# Voith ALADIN Reporter The Voith ALADIN Reporter is the central display tool for ECU files. During vehicle diagnosis, the "Upload" function reads out all the relevant data from a transmission control unit and saves it in an ECU file. The Reporter creates and ALADIN ECU report from an ECU file.
| How to open the Reporter:
The Reporter symbol has been created automatically on your desktop during the installation. Double-click the desktop symbol to start the program. Alternatively, you can open the Reporter using the Start menu. To do so, click: Start > Programs > Voith Diagnostic Tools > Voith Reporter.
| How to create an ECU report:
Navigate to the Open ECU file button in the menu. Reporter > Open ECU file. The "Open" dialog appears. Select an ECU file and confirm with Open. The ECU report is created. Alternatively, click . The "Open" dialog appears. Select an ECU file and confirm with Open. The ECU report is created. For further information on ECU reports, please see: ALADIN ECU report.
| Functions of the Reporter
> In addition to the ALADIN ECU report, the Voith Reporter includes the following functions:
> Clone ECU file | Function for creating an equivalent control unit on the basis of an ECU file. For further information, please see: Cloning. |
> Export of event lists | Creates complete event memory lists. For further information, please see: Export of event lists. |
> Operating data report | Creates a difference report between different ECU files. For further information, please see: Operating data report. |
| Adjust ECU report contents:
In the ALADIN Setup, you can configure what is displayed and how it is displayed in the ECU report. Open the setup by clicking: Reporter > Settings. For further information, please see: Report setup.
| Further topics:
More information on: Report More information on: Upload More information on: FAQ Up > Higher-level section © by Voith Turbo GmbH & Co. KG send remarks to joachim.ehleiter@voith.com (electronic department) or r.theilacker@voith.com (electronic department)