Start page To favorites Print page |

### Service - Transmission monitor

In the Transmission monitor, you can monitor the current status of all sensors, solenoid valves, digital input/output signals and control elements in real time. For this purpose, the Monitor window is divided into the following tabs:

- Sensors
- Speeds
- Control elements
- Actuators
- Digital IO
- Texts

## Valid platforms:

- DIWA.3 via E200
- DIWA.3 via E310
- DIWA.5
- DIWA.6 via KWP
- DIWAhybrid E300.1

The transmission monitor is accessed via the Service group in the main window. Then select the Transmission monitor button in the Service menu.

The transmission monitor is offered depending on the connected ECU. No functions are available without communication.

The display changes automatically after you have started the communication.
The measurement values are displayed depending on the connected controller.